**Nucor Box 27 Notes**

(Use these when Processing an order, or defining on a Scope Sheet, for Pricing and Production)

1. Provide J-Trim (HTD-\_\_\_) instead of Nucor Standard window sill trims, on windows that are furnished with nailing flanges.
2. Nucor to provide foam closures at base conditions, framed opening headers and sills, eave conditions and panel splice locations at wainscoting.
3. Provide a galvanized angle at the roof to sidewall and roof to endwall intersections on the interior girt faces, for simple saver insulation vapor barrier fabric attachment. (priced at $1.00/lf, added to program pricing)(Refer to Nucor detail, “Section 10”, Liner Panel, Partition Wall and Draft Curtain Details I00010.DWG))